set_property BITSTREAM.CONFIG.UNUSEDPIN PULLNONE [current_design]

#### ===========================================================================
#### USR
#### ===========================================================================

set_property -dict {PACKAGE_PIN AE10 IOSTANDARD LVCMOS33} [get_ports {USR_tri_io[0]}]
set_property -dict {PACKAGE_PIN AF10 IOSTANDARD LVCMOS33} [get_ports {USR_tri_io[1]}]
set_property -dict {PACKAGE_PIN AE12 IOSTANDARD LVCMOS33} [get_ports {USR_tri_io[2]}]
set_property -dict {PACKAGE_PIN AF12 IOSTANDARD LVCMOS33} [get_ports {USR_tri_io[3]}]
set_property -dict {PACKAGE_PIN AE13 IOSTANDARD LVCMOS33} [get_ports {USR_tri_io[4]}]
set_property -dict {PACKAGE_PIN AF13 IOSTANDARD LVCMOS33} [get_ports {USR_tri_io[5]}]
set_property -dict {PACKAGE_PIN AF14 IOSTANDARD LVCMOS33} [get_ports {USR_tri_io[6]}]
set_property -dict {PACKAGE_PIN AD14 IOSTANDARD LVCMOS33} [get_ports {USR_tri_io[7]}]
set_property -dict {PACKAGE_PIN AD13 IOSTANDARD LVCMOS33} [get_ports {USR_tri_io[8]}]
set_property -dict {PACKAGE_PIN AC14 IOSTANDARD LVCMOS33} [get_ports {USR_tri_io[9]}]
set_property -dict {PACKAGE_PIN Y16  IOSTANDARD LVCMOS33} [get_ports {USR_tri_io[10]}]
set_property -dict {PACKAGE_PIN AD15 IOSTANDARD LVCMOS33} [get_ports {USR_tri_io[11]}]
set_property -dict {PACKAGE_PIN AC16 IOSTANDARD LVCMOS33} [get_ports {USR_tri_io[12]}]
set_property -dict {PACKAGE_PIN AD16 IOSTANDARD LVCMOS33} [get_ports {USR_tri_io[13]}]
set_property -dict {PACKAGE_PIN AA17 IOSTANDARD LVCMOS33} [get_ports {USR_tri_io[14]}]
set_property -dict {PACKAGE_PIN AC17 IOSTANDARD LVCMOS33} [get_ports {USR_tri_io[15]}]
set_property -dict {PACKAGE_PIN AA12 IOSTANDARD LVCMOS33} [get_ports {USR_tri_io[16]}]
set_property -dict {PACKAGE_PIN AA13 IOSTANDARD LVCMOS33} [get_ports {USR_tri_io[17]}]
set_property -dict {PACKAGE_PIN AA14 IOSTANDARD LVCMOS33} [get_ports {USR_tri_io[18]}]
set_property -dict {PACKAGE_PIN AA15 IOSTANDARD LVCMOS33} [get_ports {USR_tri_io[19]}]
set_property -dict {PACKAGE_PIN AC13 IOSTANDARD LVCMOS33} [get_ports {USR_tri_io[20]}]
set_property -dict {PACKAGE_PIN W13  IOSTANDARD LVCMOS33} [get_ports {USR_tri_io[21]}]
set_property -dict {PACKAGE_PIN W14  IOSTANDARD LVCMOS33} [get_ports {USR_tri_io[22]}]
set_property -dict {PACKAGE_PIN AB14 IOSTANDARD LVCMOS33} [get_ports {USR_tri_io[23]}]
set_property -dict {PACKAGE_PIN Y13  IOSTANDARD LVCMOS33} [get_ports {USR_tri_io[24]}]
set_property -dict {PACKAGE_PIN Y15  IOSTANDARD LVCMOS33} [get_ports {USR_tri_io[25]}]
set_property -dict {PACKAGE_PIN W15  IOSTANDARD LVCMOS33} [get_ports {USR_tri_io[26]}]
set_property -dict {PACKAGE_PIN W16  IOSTANDARD LVCMOS33} [get_ports {USR_tri_io[27]}]
set_property -dict {PACKAGE_PIN AB15 IOSTANDARD LVCMOS33} [get_ports {USR_tri_io[28]}]
set_property -dict {PACKAGE_PIN AB16 IOSTANDARD LVCMOS33} [get_ports {USR_tri_io[29]}]
set_property -dict {PACKAGE_PIN AB17 IOSTANDARD LVCMOS33} [get_ports {USR_tri_io[30]}]
set_property -dict {PACKAGE_PIN Y17  IOSTANDARD LVCMOS33} [get_ports {USR_tri_io[31]}]
set_property -dict {PACKAGE_PIN AA10 IOSTANDARD LVCMOS33} [get_ports {USR_tri_io[32]}]
set_property -dict {PACKAGE_PIN AD10 IOSTANDARD LVCMOS33} [get_ports {USR_tri_io[33]}]
set_property -dict {PACKAGE_PIN AB10 IOSTANDARD LVCMOS33} [get_ports {USR_tri_io[34]}]
set_property -dict {PACKAGE_PIN Y11  IOSTANDARD LVCMOS33} [get_ports {USR_tri_io[35]}]

#### ===========================================================================
#### PWM
#### ===========================================================================

set_property -dict {PACKAGE_PIN AC22 IOSTANDARD LVCMOS33} [get_ports {pwm[0]}]
set_property -dict {PACKAGE_PIN AD23 IOSTANDARD LVCMOS33} [get_ports {pwm[1]}]
set_property -dict {PACKAGE_PIN AC23 IOSTANDARD LVCMOS33} [get_ports {pwm[2]}]
set_property -dict {PACKAGE_PIN AD24 IOSTANDARD LVCMOS33} [get_ports {pwm[3]}]
set_property -dict {PACKAGE_PIN AC24 IOSTANDARD LVCMOS33} [get_ports {pwm[4]}]
set_property -dict {PACKAGE_PIN AB24 IOSTANDARD LVCMOS33} [get_ports {pwm[5]}]
set_property -dict {PACKAGE_PIN AA24 IOSTANDARD LVCMOS33} [get_ports {pwm[6]}]
set_property -dict {PACKAGE_PIN AA25 IOSTANDARD LVCMOS33} [get_ports {pwm[7]}]
set_property -dict {PACKAGE_PIN AF25 IOSTANDARD LVCMOS33} [get_ports {pwm[8]}]
set_property -dict {PACKAGE_PIN AE25 IOSTANDARD LVCMOS33} [get_ports {pwm[9]}]
set_property -dict {PACKAGE_PIN AE26 IOSTANDARD LVCMOS33} [get_ports {pwm[10]}]
set_property -dict {PACKAGE_PIN AD25 IOSTANDARD LVCMOS33} [get_ports {pwm[11]}]
set_property -dict {PACKAGE_PIN AD26 IOSTANDARD LVCMOS33} [get_ports {pwm[12]}]
set_property -dict {PACKAGE_PIN AC26 IOSTANDARD LVCMOS33} [get_ports {pwm[13]}]
set_property -dict {PACKAGE_PIN AB25 IOSTANDARD LVCMOS33} [get_ports {pwm[14]}]
set_property -dict {PACKAGE_PIN AB26 IOSTANDARD LVCMOS33} [get_ports {pwm[15]}]
set_property -dict {PACKAGE_PIN A7   IOSTANDARD LVCMOS18} [get_ports {pwm[16]}]
set_property -dict {PACKAGE_PIN A8   IOSTANDARD LVCMOS18} [get_ports {pwm[17]}]
set_property -dict {PACKAGE_PIN B9   IOSTANDARD LVCMOS18} [get_ports {pwm[18]}]
set_property -dict {PACKAGE_PIN A9   IOSTANDARD LVCMOS18} [get_ports {pwm[19]}]
set_property -dict {PACKAGE_PIN E6   IOSTANDARD LVCMOS18} [get_ports {pwm[20]}]
set_property -dict {PACKAGE_PIN F7   IOSTANDARD LVCMOS18} [get_ports {pwm[21]}]
set_property -dict {PACKAGE_PIN E8   IOSTANDARD LVCMOS18} [get_ports {pwm[22]}]
set_property -dict {PACKAGE_PIN F9   IOSTANDARD LVCMOS18} [get_ports {pwm[23]}]
set_property -dict {PACKAGE_PIN G5   IOSTANDARD LVCMOS18} [get_ports {pwm[24]}]
set_property -dict {PACKAGE_PIN H6   IOSTANDARD LVCMOS18} [get_ports {pwm[25]}]
set_property -dict {PACKAGE_PIN H7   IOSTANDARD LVCMOS18} [get_ports {pwm[26]}]
set_property -dict {PACKAGE_PIN H8   IOSTANDARD LVCMOS18} [get_ports {pwm[27]}]
set_property -dict {PACKAGE_PIN A12  IOSTANDARD LVCMOS18} [get_ports {pwm[28]}]
set_property -dict {PACKAGE_PIN J10  IOSTANDARD LVCMOS18} [get_ports {pwm[29]}]
set_property -dict {PACKAGE_PIN H11  IOSTANDARD LVCMOS18} [get_ports {pwm[30]}]
set_property -dict {PACKAGE_PIN J11  IOSTANDARD LVCMOS18} [get_ports {pwm[31]}]

#### ===========================================================================
#### GPO
#### ===========================================================================

set_property -dict {PACKAGE_PIN AF24 IOSTANDARD LVCMOS33} [get_ports {gpo[0]}]
set_property -dict {PACKAGE_PIN AE23 IOSTANDARD LVCMOS33} [get_ports {gpo[1]}]
set_property -dict {PACKAGE_PIN AF23 IOSTANDARD LVCMOS33} [get_ports {gpo[2]}]
set_property -dict {PACKAGE_PIN AE22 IOSTANDARD LVCMOS33} [get_ports {gpo[3]}]
set_property -dict {PACKAGE_PIN AF22 IOSTANDARD LVCMOS33} [get_ports {gpo[4]}]
set_property -dict {PACKAGE_PIN AE21 IOSTANDARD LVCMOS33} [get_ports {gpo[5]}]
set_property -dict {PACKAGE_PIN AE20 IOSTANDARD LVCMOS33} [get_ports {gpo[6]}]
set_property -dict {PACKAGE_PIN AF20 IOSTANDARD LVCMOS33} [get_ports {gpo[7]}]
set_property -dict {PACKAGE_PIN B7   IOSTANDARD LVCMOS18} [get_ports {gpo[8]}]
set_property -dict {PACKAGE_PIN B6   IOSTANDARD LVCMOS18} [get_ports {gpo[9]}]
set_property -dict {PACKAGE_PIN A5   IOSTANDARD LVCMOS18} [get_ports {gpo[10]}]
set_property -dict {PACKAGE_PIN B5   IOSTANDARD LVCMOS18} [get_ports {gpo[11]}]
set_property -dict {PACKAGE_PIN A4   IOSTANDARD LVCMOS18} [get_ports {gpo[12]}]
set_property -dict {PACKAGE_PIN A3   IOSTANDARD LVCMOS18} [get_ports {gpo[13]}]
set_property -dict {PACKAGE_PIN A2   IOSTANDARD LVCMOS18} [get_ports {gpo[14]}]
set_property -dict {PACKAGE_PIN B1   IOSTANDARD LVCMOS18} [get_ports {gpo[15]}]

#### ===========================================================================
#### GPI
#### ===========================================================================

set_property -dict {PACKAGE_PIN AA23 IOSTANDARD LVCMOS33 PULLDOWN TRUE} [get_ports gpi[0]]
set_property -dict {PACKAGE_PIN AB22 IOSTANDARD LVCMOS33 PULLDOWN TRUE} [get_ports gpi[1]]
set_property -dict {PACKAGE_PIN AA22 IOSTANDARD LVCMOS33 PULLDOWN TRUE} [get_ports gpi[2]]
set_property -dict {PACKAGE_PIN AB21 IOSTANDARD LVCMOS33 PULLDOWN TRUE} [get_ports gpi[3]]
set_property -dict {PACKAGE_PIN W20  IOSTANDARD LVCMOS33 PULLDOWN TRUE} [get_ports gpi[4]]
set_property -dict {PACKAGE_PIN Y18  IOSTANDARD LVCMOS33 PULLDOWN TRUE} [get_ports gpi[5]]
set_property -dict {PACKAGE_PIN W19  IOSTANDARD LVCMOS33 PULLDOWN TRUE} [get_ports gpi[6]]
set_property -dict {PACKAGE_PIN W18  IOSTANDARD LVCMOS33 PULLDOWN TRUE} [get_ports gpi[7]]
set_property -dict {PACKAGE_PIN F2   IOSTANDARD LVCMOS18}               [get_ports gpi[8]]
set_property -dict {PACKAGE_PIN G2   IOSTANDARD LVCMOS18}               [get_ports gpi[9]]
set_property -dict {PACKAGE_PIN G1   IOSTANDARD LVCMOS18}               [get_ports gpi[10]]
set_property -dict {PACKAGE_PIN H2   IOSTANDARD LVCMOS18}               [get_ports gpi[11]]
set_property -dict {PACKAGE_PIN H1   IOSTANDARD LVCMOS18}               [get_ports gpi[12]]
set_property -dict {PACKAGE_PIN J1   IOSTANDARD LVCMOS18}               [get_ports gpi[13]]
set_property -dict {PACKAGE_PIN K2   IOSTANDARD LVCMOS18}               [get_ports gpi[14]]
set_property -dict {PACKAGE_PIN K1   IOSTANDARD LVCMOS18}               [get_ports gpi[15]]

#### ===========================================================================
#### FLT/DIN
#### ===========================================================================

set_property -dict {PACKAGE_PIN B4 IOSTANDARD LVCMOS18 PULLDOWN TRUE} [get_ports flt[0]]
set_property -dict {PACKAGE_PIN E5 IOSTANDARD LVCMOS18 PULLDOWN TRUE} [get_ports flt[1]]
set_property -dict {PACKAGE_PIN D6 IOSTANDARD LVCMOS18 PULLDOWN TRUE} [get_ports flt[2]]
set_property -dict {PACKAGE_PIN E7 IOSTANDARD LVCMOS18 PULLDOWN TRUE} [get_ports flt[3]]
set_property -dict {PACKAGE_PIN C6 IOSTANDARD LVCMOS18 PULLDOWN TRUE} [get_ports flt[4]]
set_property -dict {PACKAGE_PIN F8 IOSTANDARD LVCMOS18 PULLDOWN TRUE} [get_ports flt[5]]
set_property -dict {PACKAGE_PIN C7 IOSTANDARD LVCMOS18 PULLDOWN TRUE} [get_ports flt[6]]
set_property -dict {PACKAGE_PIN G9 IOSTANDARD LVCMOS18 PULLDOWN TRUE} [get_ports flt[7]]
set_property -dict {PACKAGE_PIN B2 IOSTANDARD LVCMOS18 PULLDOWN TRUE} [get_ports flt[8]]
set_property -dict {PACKAGE_PIN C2 IOSTANDARD LVCMOS18 PULLDOWN TRUE} [get_ports flt[9]]
set_property -dict {PACKAGE_PIN D5 IOSTANDARD LVCMOS18 PULLDOWN TRUE} [get_ports flt[10]]
set_property -dict {PACKAGE_PIN F5 IOSTANDARD LVCMOS18 PULLDOWN TRUE} [get_ports flt[11]]
set_property -dict {PACKAGE_PIN G6 IOSTANDARD LVCMOS18 PULLDOWN TRUE} [get_ports flt[12]]
set_property -dict {PACKAGE_PIN G7 IOSTANDARD LVCMOS18 PULLDOWN TRUE} [get_ports flt[13]]
set_property -dict {PACKAGE_PIN J8 IOSTANDARD LVCMOS18 PULLDOWN TRUE} [get_ports flt[14]]
set_property -dict {PACKAGE_PIN C8 IOSTANDARD LVCMOS18 PULLDOWN TRUE} [get_ports flt[15]]

#### ===========================================================================
#### B-BOX
#### ===========================================================================

set_property -dict {PACKAGE_PIN D13 IOSTANDARD LVCMOS18} [get_ports {BBOX_tri_io[0]}]
set_property -dict {PACKAGE_PIN D14 IOSTANDARD LVCMOS18} [get_ports {BBOX_tri_io[1]}]
set_property -dict {PACKAGE_PIN E13 IOSTANDARD LVCMOS18} [get_ports {BBOX_tri_io[2]}]
set_property -dict {PACKAGE_PIN C14 IOSTANDARD LVCMOS18} [get_ports {BBOX_tri_io[3]}]
set_property -dict {PACKAGE_PIN D15 IOSTANDARD LVCMOS18} [get_ports {BBOX_tri_io[4]}]
set_property -dict {PACKAGE_PIN A17 IOSTANDARD LVCMOS18} [get_ports {BBOX_tri_io[5]}]
set_property -dict {PACKAGE_PIN B17 IOSTANDARD LVCMOS18} [get_ports {BBOX_tri_io[6]}]
set_property -dict {PACKAGE_PIN E16 IOSTANDARD LVCMOS18} [get_ports {BBOX_tri_io[7]}]
set_property -dict {PACKAGE_PIN C16 IOSTANDARD LVCMOS18} [get_ports {BBOX_tri_io[8]}]
set_property -dict {PACKAGE_PIN C17 IOSTANDARD LVCMOS18} [get_ports {BBOX_tri_io[9]}]
set_property -dict {PACKAGE_PIN G10 IOSTANDARD LVCMOS18} [get_ports {BBOX_tri_io[10]}]
set_property -dict {PACKAGE_PIN K12 IOSTANDARD LVCMOS18} [get_ports {BBOX_tri_io[11]}]
set_property -dict {PACKAGE_PIN K13 IOSTANDARD LVCMOS18} [get_ports {BBOX_tri_io[12]}]
set_property -dict {PACKAGE_PIN H13 IOSTANDARD LVCMOS18} [get_ports {BBOX_tri_io[13]}]
set_property -dict {PACKAGE_PIN F14 IOSTANDARD LVCMOS18} [get_ports {BBOX_tri_io[14]}]
set_property -dict {PACKAGE_PIN F15 IOSTANDARD LVCMOS18} [get_ports {BBOX_tri_io[15]}]
set_property -dict {PACKAGE_PIN E15 IOSTANDARD LVCMOS18} [get_ports {BBOX_tri_io[16]}]
set_property -dict {PACKAGE_PIN G15 IOSTANDARD LVCMOS18} [get_ports {BBOX_tri_io[17]}]
set_property -dict {PACKAGE_PIN J14 IOSTANDARD LVCMOS18} [get_ports {BBOX_tri_io[18]}]
set_property -dict {PACKAGE_PIN J15 IOSTANDARD LVCMOS18} [get_ports {BBOX_tri_io[19]}]
set_property -dict {PACKAGE_PIN K15 IOSTANDARD LVCMOS18} [get_ports {BBOX_tri_io[20]}]
set_property -dict {PACKAGE_PIN D16 IOSTANDARD LVCMOS18} [get_ports {BBOX_tri_io[21]}]
set_property -dict {PACKAGE_PIN D11 IOSTANDARD LVCMOS18} [get_ports {BBOX_tri_io[22]}]
set_property -dict {PACKAGE_PIN J13 IOSTANDARD LVCMOS18} [get_ports {BBOX_tri_io[23]}]
set_property -dict {PACKAGE_PIN G11 IOSTANDARD LVCMOS18} [get_ports {BBOX_tri_io[24]}]
set_property -dict {PACKAGE_PIN F12 IOSTANDARD LVCMOS18} [get_ports {BBOX_tri_io[25]}]
set_property -dict {PACKAGE_PIN C13 IOSTANDARD LVCMOS18} [get_ports {BBOX_tri_io[26]}]
set_property -dict {PACKAGE_PIN E12 IOSTANDARD LVCMOS18} [get_ports {BBOX_tri_io[27]}]
set_property -dict {PACKAGE_PIN D10 IOSTANDARD LVCMOS18} [get_ports {BBOX_tri_io[28]}]
set_property -dict {PACKAGE_PIN E11 IOSTANDARD LVCMOS18} [get_ports {BBOX_tri_io[29]}]
set_property -dict {PACKAGE_PIN C11 IOSTANDARD LVCMOS18} [get_ports {BBOX_tri_io[30]}]
set_property -dict {PACKAGE_PIN H12 IOSTANDARD LVCMOS18} [get_ports {BBOX_tri_io[31]}]
set_property -dict {PACKAGE_PIN F13 IOSTANDARD LVCMOS18} [get_ports {BBOX_tri_io[32]}]
set_property -dict {PACKAGE_PIN G12 IOSTANDARD LVCMOS18} [get_ports {BBOX_tri_io[33]}]
set_property -dict {PACKAGE_PIN A13 IOSTANDARD LVCMOS18} [get_ports {BBOX_tri_io[34]}]
set_property -dict {PACKAGE_PIN A14 IOSTANDARD LVCMOS18} [get_ports {BBOX_tri_io[35]}]
set_property -dict {PACKAGE_PIN B14 IOSTANDARD LVCMOS18} [get_ports {BBOX_tri_io[36]}]
set_property -dict {PACKAGE_PIN A15 IOSTANDARD LVCMOS18} [get_ports {BBOX_tri_io[37]}]
set_property -dict {PACKAGE_PIN B15 IOSTANDARD LVCMOS18} [get_ports {BBOX_tri_io[38]}]
set_property -dict {PACKAGE_PIN B16 IOSTANDARD LVCMOS18} [get_ports {BBOX_tri_io[39]}]
set_property -dict {PACKAGE_PIN H14 IOSTANDARD LVCMOS18} [get_ports {BBOX_tri_io[40]}]
set_property -dict {PACKAGE_PIN G14 IOSTANDARD LVCMOS18} [get_ports {BBOX_tri_io[41]}]
set_property -dict {PACKAGE_PIN H16 IOSTANDARD LVCMOS18} [get_ports {BBOX_tri_io[42]}]
set_property -dict {PACKAGE_PIN G16 IOSTANDARD LVCMOS18} [get_ports {BBOX_tri_io[43]}]
set_property -dict {PACKAGE_PIN E10 IOSTANDARD LVCMOS18} [get_ports {BBOX_tri_io[44]}]
set_property -dict {PACKAGE_PIN F10 IOSTANDARD LVCMOS18} [get_ports {BBOX_tri_io[45]}]
set_property -dict {PACKAGE_PIN B11 IOSTANDARD LVCMOS18} [get_ports {BBOX_tri_io[46]}]
set_property -dict {PACKAGE_PIN B12 IOSTANDARD LVCMOS18} [get_ports {BBOX_tri_io[47]}]
set_property -dict {PACKAGE_PIN C3  IOSTANDARD LVCMOS18} [get_ports {BBOX_tri_io[48]}]
set_property -dict {PACKAGE_PIN C4  IOSTANDARD LVCMOS18} [get_ports {BBOX_tri_io[49]}]
set_property -dict {PACKAGE_PIN D9  IOSTANDARD LVCMOS18} [get_ports {BBOX_tri_io[50]}]
set_property -dict {PACKAGE_PIN D8  IOSTANDARD LVCMOS18} [get_ports {BBOX_tri_io[51]}]

#### ===========================================================================
#### VHDCA
#### ===========================================================================

#set_property -dict {PACKAGE_PIN A10 IOSTANDARD LVCMOS18} [get_ports {vhdca[0]}]
#set_property -dict {PACKAGE_PIN B10 IOSTANDARD LVCMOS18} [get_ports {vhdca[1]}]
#set_property -dict {PACKAGE_PIN J9  IOSTANDARD LVCMOS18} [get_ports {vhdca[2]}]
#set_property -dict {PACKAGE_PIN C9  IOSTANDARD LVCMOS18} [get_ports {vhdca[3]}]

#### ===========================================================================
#### PRIVATE
#### ===========================================================================

set_property PACKAGE_PIN R2  [get_ports {private_out[28]}]
set_property PACKAGE_PIN R1  [get_ports {private_out[29]}]
set_property PACKAGE_PIN U2  [get_ports {private_out[30]}]
set_property PACKAGE_PIN U1  [get_ports {private_out[31]}]
set_property PACKAGE_PIN W2  [get_ports {private_out[32]}]
set_property PACKAGE_PIN W1  [get_ports {private_out[33]}]
set_property PACKAGE_PIN AA2 [get_ports {private_out[34]}]
set_property PACKAGE_PIN AA1 [get_ports {private_out[35]}]
set_property PACKAGE_PIN T4  [get_ports {private_in[23]}]
set_property PACKAGE_PIN T3  [get_ports {private_in[24]}]
set_property PACKAGE_PIN V4  [get_ports {private_in[25]}]
set_property PACKAGE_PIN V3  [get_ports {private_in[26]}]
set_property PACKAGE_PIN Y4  [get_ports {private_in[27]}]
set_property PACKAGE_PIN Y3  [get_ports {private_in[28]}]
set_property PACKAGE_PIN AB4 [get_ports {private_in[29]}]
set_property PACKAGE_PIN AB3 [get_ports {private_in[30]}]
create_clock -period 4.000 -name {private_in[21]} -waveform {0.000 2.000} [get_ports {private_in[21]}]
set_property PACKAGE_PIN R6 [get_ports {private_in[21]}]
set_property PACKAGE_PIN R5 [get_ports {private_in[22]}]
set_property -dict {PACKAGE_PIN AD20 IOSTANDARD LVCMOS33} [get_ports {private_out[0]}]
set_property -dict {PACKAGE_PIN AC19 IOSTANDARD LVCMOS33} [get_ports {private_out[1]}]
set_property -dict {PACKAGE_PIN AD21 IOSTANDARD LVCMOS33 PULLUP true} [get_ports {private_out[2]}]
set_property -dict {PACKAGE_PIN AA19 IOSTANDARD LVCMOS33} [get_ports {private_in[16]}]
set_property -dict {PACKAGE_PIN M6 IOSTANDARD LVDS} [get_ports {private_out[3]}]
set_property -dict {PACKAGE_PIN M5 IOSTANDARD LVDS} [get_ports {private_out[4]}]
set_property -dict {PACKAGE_PIN J4 IOSTANDARD LVDS} [get_ports {private_out[5]}]
set_property -dict {PACKAGE_PIN J3 IOSTANDARD LVDS} [get_ports {private_out[6]}]
set_property -dict {PACKAGE_PIN H3 IOSTANDARD LVCMOS18} [get_ports {private_out[7]}]
set_property -dict {PACKAGE_PIN N8 IOSTANDARD LVCMOS18 SLEW FAST} [get_ports {private_out[8]}]
set_property -dict {PACKAGE_PIN M8 IOSTANDARD LVCMOS18} [get_ports {private_in[0]}]
set_property -dict {PACKAGE_PIN M7 IOSTANDARD LVCMOS18} [get_ports {private_in[1]}]
set_property -dict {PACKAGE_PIN K7 IOSTANDARD LVCMOS18} [get_ports {private_in[2]}]
set_property -dict {PACKAGE_PIN H4 IOSTANDARD LVCMOS18} [get_ports {private_in[3]}]
set_property -dict {PACKAGE_PIN L3 IOSTANDARD LVCMOS18} [get_ports {private_in[4]}]
create_clock -period 9.000 -name {private_in[4]} -waveform {0.000 4.500} [get_ports {private_in[4]}]
set_property -dict {PACKAGE_PIN J5 IOSTANDARD LVCMOS18} [get_ports {private_out[9]}]
set_property -dict {PACKAGE_PIN N3 IOSTANDARD LVCMOS18 SLEW FAST} [get_ports {private_out[10]}]
set_property -dict {PACKAGE_PIN N4 IOSTANDARD LVCMOS18} [get_ports {private_in[5]}]
set_property -dict {PACKAGE_PIN L7 IOSTANDARD LVCMOS18} [get_ports {private_in[6]}]
set_property -dict {PACKAGE_PIN K6 IOSTANDARD LVCMOS18} [get_ports {private_in[7]}]
set_property -dict {PACKAGE_PIN J6 IOSTANDARD LVCMOS18} [get_ports {private_in[8]}]
set_property -dict {PACKAGE_PIN L5 IOSTANDARD LVCMOS18} [get_ports {private_in[9]}]
create_clock -period 9.000 -name {private_in[9]} -waveform {0.000 4.500} [get_ports {private_in[9]}]
set_property -dict {PACKAGE_PIN K11 IOSTANDARD LVCMOS18} [get_ports {private_out[11]}]
set_property -dict {PACKAGE_PIN E1 IOSTANDARD LVCMOS18} [get_ports {private_out[12]}]
set_property -dict {PACKAGE_PIN AE15 IOSTANDARD LVCMOS33 PULLUP true}   [get_ports {private_out[13]}]
set_property -dict {PACKAGE_PIN AE16 IOSTANDARD LVCMOS33 PULLUP true}   [get_ports {private_out[14]}]
set_property -dict {PACKAGE_PIN AE17 IOSTANDARD LVCMOS33 PULLUP true}   [get_ports {private_out[15]}]
set_property -dict {PACKAGE_PIN AF17 IOSTANDARD LVCMOS33 PULLUP true}   [get_ports {private_in[14]}]
set_property -dict {PACKAGE_PIN AF15 IOSTANDARD LVCMOS33 PULLDOWN true} [get_ports {private_in[15]}]
set_property -dict {PACKAGE_PIN AF18 IOSTANDARD LVCMOS33} [get_ports {private_out[16]}]
set_property -dict {PACKAGE_PIN AF19 IOSTANDARD LVCMOS33} [get_ports {private_out[17]}]
set_property -dict {PACKAGE_PIN AD18 IOSTANDARD LVCMOS33} [get_ports {private_out[18]}]
set_property -dict {PACKAGE_PIN AA18 IOSTANDARD LVCMOS33} [get_ports {private_out[19]}]
set_property -dict {PACKAGE_PIN AB19 IOSTANDARD LVCMOS33} [get_ports {private_out[20]}]
set_property -dict {PACKAGE_PIN AE18 IOSTANDARD LVCMOS33} [get_ports {private_in[13]}]
set_property -dict {PACKAGE_PIN AB11 IOSTANDARD LVCMOS33} [get_ports {private_out[21]}]
set_property -dict {PACKAGE_PIN AC11 IOSTANDARD LVCMOS33} [get_ports {private_in[10]}]
set_property -dict {PACKAGE_PIN AC12 IOSTANDARD LVCMOS33 PULLDOWN true} [get_ports {private_in[11]}]
set_property -dict {PACKAGE_PIN AD11 IOSTANDARD LVCMOS33} [get_ports {private_in[12]}]
set_property -dict {PACKAGE_PIN D4 IOSTANDARD LVCMOS18} [get_ports {private_out[22]}]
set_property -dict {PACKAGE_PIN C1 IOSTANDARD LVCMOS18} [get_ports {private_out[23]}]
set_property -dict {PACKAGE_PIN D3 IOSTANDARD LVCMOS18} [get_ports {private_out[24]}]
set_property -dict {PACKAGE_PIN D1 IOSTANDARD LVCMOS18} [get_ports {private_out[25]}]
set_property -dict {PACKAGE_PIN E2 IOSTANDARD LVCMOS18} [get_ports {private_out[26]}]
set_property -dict {PACKAGE_PIN E3 IOSTANDARD LVCMOS18} [get_ports {private_out[27]}]
set_property -dict {PACKAGE_PIN K10 IOSTANDARD LVCMOS18 PULLUP true} [get_ports {private_in[20]}]
set_property -dict {PACKAGE_PIN Y10 IOSTANDARD LVCMOS33 PULLDOWN true} [get_ports {private_in[17]}]
set_property -dict {PACKAGE_PIN Y12 IOSTANDARD LVCMOS33 PULLDOWN true} [get_ports {private_in[18]}]
set_property -dict {PACKAGE_PIN AB12 IOSTANDARD LVCMOS33 PULLDOWN true} [get_ports {private_in[19]}]

