current_instance -quiet
set_property IOSTANDARD LVCMOS18 [get_ports {FIXED_IO_mio[53]}]
set_property SLEW SLOW [get_ports {FIXED_IO_mio[53]}]
set_property DRIVE 8 [get_ports {FIXED_IO_mio[53]}]
set_property PULLUP true [get_ports {FIXED_IO_mio[53]}]
set_property PIO_DIRECTION BIDIR [get_ports {FIXED_IO_mio[53]}]
set_property IOSTANDARD LVCMOS18 [get_ports {FIXED_IO_mio[52]}]
set_property SLEW SLOW [get_ports {FIXED_IO_mio[52]}]
set_property DRIVE 8 [get_ports {FIXED_IO_mio[52]}]
set_property PULLUP true [get_ports {FIXED_IO_mio[52]}]
set_property PIO_DIRECTION OUTPUT [get_ports {FIXED_IO_mio[52]}]
set_property IOSTANDARD LVCMOS18 [get_ports {FIXED_IO_mio[51]}]
set_property SLEW SLOW [get_ports {FIXED_IO_mio[51]}]
set_property DRIVE 8 [get_ports {FIXED_IO_mio[51]}]
set_property PULLUP true [get_ports {FIXED_IO_mio[51]}]
set_property PIO_DIRECTION BIDIR [get_ports {FIXED_IO_mio[51]}]
set_property IOSTANDARD LVCMOS18 [get_ports {FIXED_IO_mio[50]}]
set_property SLEW SLOW [get_ports {FIXED_IO_mio[50]}]
set_property DRIVE 8 [get_ports {FIXED_IO_mio[50]}]
set_property PULLUP true [get_ports {FIXED_IO_mio[50]}]
set_property PIO_DIRECTION BIDIR [get_ports {FIXED_IO_mio[50]}]
set_property IOSTANDARD LVCMOS18 [get_ports {FIXED_IO_mio[49]}]
set_property SLEW SLOW [get_ports {FIXED_IO_mio[49]}]
set_property DRIVE 8 [get_ports {FIXED_IO_mio[49]}]
set_property PULLUP true [get_ports {FIXED_IO_mio[49]}]
set_property PIO_DIRECTION INPUT [get_ports {FIXED_IO_mio[49]}]
set_property IOSTANDARD LVCMOS18 [get_ports {FIXED_IO_mio[48]}]
set_property SLEW SLOW [get_ports {FIXED_IO_mio[48]}]
set_property DRIVE 8 [get_ports {FIXED_IO_mio[48]}]
set_property PULLUP true [get_ports {FIXED_IO_mio[48]}]
set_property PIO_DIRECTION OUTPUT [get_ports {FIXED_IO_mio[48]}]
set_property IOSTANDARD LVCMOS18 [get_ports {FIXED_IO_mio[45]}]
set_property SLEW SLOW [get_ports {FIXED_IO_mio[45]}]
set_property DRIVE 8 [get_ports {FIXED_IO_mio[45]}]
set_property PULLUP true [get_ports {FIXED_IO_mio[45]}]
set_property PIO_DIRECTION BIDIR [get_ports {FIXED_IO_mio[45]}]
set_property IOSTANDARD LVCMOS18 [get_ports {FIXED_IO_mio[44]}]
set_property SLEW SLOW [get_ports {FIXED_IO_mio[44]}]
set_property DRIVE 8 [get_ports {FIXED_IO_mio[44]}]
set_property PULLUP true [get_ports {FIXED_IO_mio[44]}]
set_property PIO_DIRECTION BIDIR [get_ports {FIXED_IO_mio[44]}]
set_property IOSTANDARD LVCMOS18 [get_ports {FIXED_IO_mio[43]}]
set_property SLEW SLOW [get_ports {FIXED_IO_mio[43]}]
set_property DRIVE 8 [get_ports {FIXED_IO_mio[43]}]
set_property PULLUP true [get_ports {FIXED_IO_mio[43]}]
set_property PIO_DIRECTION BIDIR [get_ports {FIXED_IO_mio[43]}]
set_property IOSTANDARD LVCMOS18 [get_ports {FIXED_IO_mio[42]}]
set_property SLEW SLOW [get_ports {FIXED_IO_mio[42]}]
set_property DRIVE 8 [get_ports {FIXED_IO_mio[42]}]
set_property PULLUP true [get_ports {FIXED_IO_mio[42]}]
set_property PIO_DIRECTION BIDIR [get_ports {FIXED_IO_mio[42]}]
set_property IOSTANDARD LVCMOS18 [get_ports {FIXED_IO_mio[41]}]
set_property SLEW SLOW [get_ports {FIXED_IO_mio[41]}]
set_property DRIVE 8 [get_ports {FIXED_IO_mio[41]}]
set_property PULLUP true [get_ports {FIXED_IO_mio[41]}]
set_property PIO_DIRECTION BIDIR [get_ports {FIXED_IO_mio[41]}]
set_property IOSTANDARD LVCMOS18 [get_ports {FIXED_IO_mio[40]}]
set_property SLEW SLOW [get_ports {FIXED_IO_mio[40]}]
set_property DRIVE 8 [get_ports {FIXED_IO_mio[40]}]
set_property PULLUP true [get_ports {FIXED_IO_mio[40]}]
set_property PIO_DIRECTION BIDIR [get_ports {FIXED_IO_mio[40]}]
set_property IOSTANDARD LVCMOS18 [get_ports {FIXED_IO_mio[39]}]
set_property SLEW FAST [get_ports {FIXED_IO_mio[39]}]
set_property DRIVE 8 [get_ports {FIXED_IO_mio[39]}]
set_property PULLUP true [get_ports {FIXED_IO_mio[39]}]
set_property PIO_DIRECTION BIDIR [get_ports {FIXED_IO_mio[39]}]
set_property IOSTANDARD LVCMOS18 [get_ports {FIXED_IO_mio[38]}]
set_property SLEW FAST [get_ports {FIXED_IO_mio[38]}]
set_property DRIVE 8 [get_ports {FIXED_IO_mio[38]}]
set_property PULLUP true [get_ports {FIXED_IO_mio[38]}]
set_property PIO_DIRECTION BIDIR [get_ports {FIXED_IO_mio[38]}]
set_property IOSTANDARD LVCMOS18 [get_ports {FIXED_IO_mio[37]}]
set_property SLEW FAST [get_ports {FIXED_IO_mio[37]}]
set_property DRIVE 8 [get_ports {FIXED_IO_mio[37]}]
set_property PULLUP true [get_ports {FIXED_IO_mio[37]}]
set_property PIO_DIRECTION BIDIR [get_ports {FIXED_IO_mio[37]}]
set_property IOSTANDARD LVCMOS18 [get_ports {FIXED_IO_mio[36]}]
set_property SLEW FAST [get_ports {FIXED_IO_mio[36]}]
set_property DRIVE 8 [get_ports {FIXED_IO_mio[36]}]
set_property PULLUP true [get_ports {FIXED_IO_mio[36]}]
set_property PIO_DIRECTION INPUT [get_ports {FIXED_IO_mio[36]}]
set_property IOSTANDARD LVCMOS18 [get_ports {FIXED_IO_mio[35]}]
set_property SLEW FAST [get_ports {FIXED_IO_mio[35]}]
set_property DRIVE 8 [get_ports {FIXED_IO_mio[35]}]
set_property PULLUP true [get_ports {FIXED_IO_mio[35]}]
set_property PIO_DIRECTION BIDIR [get_ports {FIXED_IO_mio[35]}]
set_property IOSTANDARD LVCMOS18 [get_ports {FIXED_IO_mio[34]}]
set_property SLEW FAST [get_ports {FIXED_IO_mio[34]}]
set_property DRIVE 8 [get_ports {FIXED_IO_mio[34]}]
set_property PULLUP true [get_ports {FIXED_IO_mio[34]}]
set_property PIO_DIRECTION BIDIR [get_ports {FIXED_IO_mio[34]}]
set_property IOSTANDARD LVCMOS18 [get_ports {FIXED_IO_mio[33]}]
set_property SLEW FAST [get_ports {FIXED_IO_mio[33]}]
set_property DRIVE 8 [get_ports {FIXED_IO_mio[33]}]
set_property PULLUP true [get_ports {FIXED_IO_mio[33]}]
set_property PIO_DIRECTION BIDIR [get_ports {FIXED_IO_mio[33]}]
set_property IOSTANDARD LVCMOS18 [get_ports {FIXED_IO_mio[32]}]
set_property SLEW FAST [get_ports {FIXED_IO_mio[32]}]
set_property DRIVE 8 [get_ports {FIXED_IO_mio[32]}]
set_property PULLUP true [get_ports {FIXED_IO_mio[32]}]
set_property PIO_DIRECTION BIDIR [get_ports {FIXED_IO_mio[32]}]
set_property IOSTANDARD LVCMOS18 [get_ports {FIXED_IO_mio[31]}]
set_property SLEW FAST [get_ports {FIXED_IO_mio[31]}]
set_property DRIVE 8 [get_ports {FIXED_IO_mio[31]}]
set_property PULLUP true [get_ports {FIXED_IO_mio[31]}]
set_property PIO_DIRECTION INPUT [get_ports {FIXED_IO_mio[31]}]
set_property IOSTANDARD LVCMOS18 [get_ports {FIXED_IO_mio[30]}]
set_property SLEW FAST [get_ports {FIXED_IO_mio[30]}]
set_property DRIVE 8 [get_ports {FIXED_IO_mio[30]}]
set_property PULLUP true [get_ports {FIXED_IO_mio[30]}]
set_property PIO_DIRECTION OUTPUT [get_ports {FIXED_IO_mio[30]}]
set_property IOSTANDARD LVCMOS18 [get_ports {FIXED_IO_mio[29]}]
set_property SLEW FAST [get_ports {FIXED_IO_mio[29]}]
set_property DRIVE 8 [get_ports {FIXED_IO_mio[29]}]
set_property PULLUP true [get_ports {FIXED_IO_mio[29]}]
set_property PIO_DIRECTION INPUT [get_ports {FIXED_IO_mio[29]}]
set_property IOSTANDARD LVCMOS18 [get_ports {FIXED_IO_mio[28]}]
set_property SLEW FAST [get_ports {FIXED_IO_mio[28]}]
set_property DRIVE 8 [get_ports {FIXED_IO_mio[28]}]
set_property PULLUP true [get_ports {FIXED_IO_mio[28]}]
set_property PIO_DIRECTION BIDIR [get_ports {FIXED_IO_mio[28]}]
set_property IOSTANDARD LVCMOS18 [get_ports {FIXED_IO_mio[27]}]
set_property SLEW FAST [get_ports {FIXED_IO_mio[27]}]
set_property DRIVE 8 [get_ports {FIXED_IO_mio[27]}]
set_property PULLUP true [get_ports {FIXED_IO_mio[27]}]
set_property PIO_DIRECTION INPUT [get_ports {FIXED_IO_mio[27]}]
set_property IOSTANDARD LVCMOS18 [get_ports {FIXED_IO_mio[26]}]
set_property SLEW FAST [get_ports {FIXED_IO_mio[26]}]
set_property DRIVE 8 [get_ports {FIXED_IO_mio[26]}]
set_property PULLUP true [get_ports {FIXED_IO_mio[26]}]
set_property PIO_DIRECTION INPUT [get_ports {FIXED_IO_mio[26]}]
set_property IOSTANDARD LVCMOS18 [get_ports {FIXED_IO_mio[25]}]
set_property SLEW FAST [get_ports {FIXED_IO_mio[25]}]
set_property DRIVE 8 [get_ports {FIXED_IO_mio[25]}]
set_property PULLUP true [get_ports {FIXED_IO_mio[25]}]
set_property PIO_DIRECTION INPUT [get_ports {FIXED_IO_mio[25]}]
set_property IOSTANDARD LVCMOS18 [get_ports {FIXED_IO_mio[24]}]
set_property SLEW FAST [get_ports {FIXED_IO_mio[24]}]
set_property DRIVE 8 [get_ports {FIXED_IO_mio[24]}]
set_property PULLUP true [get_ports {FIXED_IO_mio[24]}]
set_property PIO_DIRECTION INPUT [get_ports {FIXED_IO_mio[24]}]
set_property IOSTANDARD LVCMOS18 [get_ports {FIXED_IO_mio[23]}]
set_property SLEW FAST [get_ports {FIXED_IO_mio[23]}]
set_property DRIVE 8 [get_ports {FIXED_IO_mio[23]}]
set_property PULLUP true [get_ports {FIXED_IO_mio[23]}]
set_property PIO_DIRECTION INPUT [get_ports {FIXED_IO_mio[23]}]
set_property IOSTANDARD LVCMOS18 [get_ports {FIXED_IO_mio[22]}]
set_property SLEW FAST [get_ports {FIXED_IO_mio[22]}]
set_property DRIVE 8 [get_ports {FIXED_IO_mio[22]}]
set_property PULLUP true [get_ports {FIXED_IO_mio[22]}]
set_property PIO_DIRECTION INPUT [get_ports {FIXED_IO_mio[22]}]
set_property IOSTANDARD LVCMOS18 [get_ports {FIXED_IO_mio[21]}]
set_property SLEW FAST [get_ports {FIXED_IO_mio[21]}]
set_property DRIVE 8 [get_ports {FIXED_IO_mio[21]}]
set_property PULLUP true [get_ports {FIXED_IO_mio[21]}]
set_property PIO_DIRECTION OUTPUT [get_ports {FIXED_IO_mio[21]}]
set_property IOSTANDARD LVCMOS18 [get_ports {FIXED_IO_mio[20]}]
set_property SLEW FAST [get_ports {FIXED_IO_mio[20]}]
set_property DRIVE 8 [get_ports {FIXED_IO_mio[20]}]
set_property PULLUP true [get_ports {FIXED_IO_mio[20]}]
set_property PIO_DIRECTION OUTPUT [get_ports {FIXED_IO_mio[20]}]
set_property IOSTANDARD LVCMOS18 [get_ports {FIXED_IO_mio[19]}]
set_property SLEW FAST [get_ports {FIXED_IO_mio[19]}]
set_property DRIVE 8 [get_ports {FIXED_IO_mio[19]}]
set_property PULLUP true [get_ports {FIXED_IO_mio[19]}]
set_property PIO_DIRECTION OUTPUT [get_ports {FIXED_IO_mio[19]}]
set_property IOSTANDARD LVCMOS18 [get_ports {FIXED_IO_mio[18]}]
set_property SLEW FAST [get_ports {FIXED_IO_mio[18]}]
set_property DRIVE 8 [get_ports {FIXED_IO_mio[18]}]
set_property PULLUP true [get_ports {FIXED_IO_mio[18]}]
set_property PIO_DIRECTION OUTPUT [get_ports {FIXED_IO_mio[18]}]
set_property IOSTANDARD LVCMOS18 [get_ports {FIXED_IO_mio[17]}]
set_property SLEW FAST [get_ports {FIXED_IO_mio[17]}]
set_property DRIVE 8 [get_ports {FIXED_IO_mio[17]}]
set_property PULLUP true [get_ports {FIXED_IO_mio[17]}]
set_property PIO_DIRECTION OUTPUT [get_ports {FIXED_IO_mio[17]}]
set_property IOSTANDARD LVCMOS18 [get_ports {FIXED_IO_mio[16]}]
set_property SLEW FAST [get_ports {FIXED_IO_mio[16]}]
set_property DRIVE 8 [get_ports {FIXED_IO_mio[16]}]
set_property PULLUP true [get_ports {FIXED_IO_mio[16]}]
set_property PIO_DIRECTION OUTPUT [get_ports {FIXED_IO_mio[16]}]
set_property IOSTANDARD LVCMOS33 [get_ports {FIXED_IO_mio[15]}]
set_property SLEW SLOW [get_ports {FIXED_IO_mio[15]}]
set_property DRIVE 8 [get_ports {FIXED_IO_mio[15]}]
set_property PULLUP true [get_ports {FIXED_IO_mio[15]}]
set_property PIO_DIRECTION BIDIR [get_ports {FIXED_IO_mio[15]}]
set_property IOSTANDARD LVCMOS33 [get_ports {FIXED_IO_mio[14]}]
set_property SLEW SLOW [get_ports {FIXED_IO_mio[14]}]
set_property DRIVE 8 [get_ports {FIXED_IO_mio[14]}]
set_property PULLUP true [get_ports {FIXED_IO_mio[14]}]
set_property PIO_DIRECTION BIDIR [get_ports {FIXED_IO_mio[14]}]
set_property IOSTANDARD LVCMOS33 [get_ports {FIXED_IO_mio[13]}]
set_property SLEW SLOW [get_ports {FIXED_IO_mio[13]}]
set_property DRIVE 8 [get_ports {FIXED_IO_mio[13]}]
set_property PULLUP true [get_ports {FIXED_IO_mio[13]}]
set_property PIO_DIRECTION BIDIR [get_ports {FIXED_IO_mio[13]}]
set_property IOSTANDARD LVCMOS33 [get_ports {FIXED_IO_mio[12]}]
set_property SLEW SLOW [get_ports {FIXED_IO_mio[12]}]
set_property DRIVE 8 [get_ports {FIXED_IO_mio[12]}]
set_property PULLUP true [get_ports {FIXED_IO_mio[12]}]
set_property PIO_DIRECTION BIDIR [get_ports {FIXED_IO_mio[12]}]
set_property IOSTANDARD LVCMOS33 [get_ports {FIXED_IO_mio[11]}]
set_property SLEW SLOW [get_ports {FIXED_IO_mio[11]}]
set_property DRIVE 8 [get_ports {FIXED_IO_mio[11]}]
set_property PULLUP true [get_ports {FIXED_IO_mio[11]}]
set_property PIO_DIRECTION BIDIR [get_ports {FIXED_IO_mio[11]}]
set_property IOSTANDARD LVCMOS33 [get_ports {FIXED_IO_mio[10]}]
set_property SLEW SLOW [get_ports {FIXED_IO_mio[10]}]
set_property DRIVE 8 [get_ports {FIXED_IO_mio[10]}]
set_property PULLUP true [get_ports {FIXED_IO_mio[10]}]
set_property PIO_DIRECTION BIDIR [get_ports {FIXED_IO_mio[10]}]
set_property IOSTANDARD LVCMOS33 [get_ports {FIXED_IO_mio[9]}]
set_property SLEW SLOW [get_ports {FIXED_IO_mio[9]}]
set_property DRIVE 8 [get_ports {FIXED_IO_mio[9]}]
set_property PULLUP true [get_ports {FIXED_IO_mio[9]}]
set_property PIO_DIRECTION INPUT [get_ports {FIXED_IO_mio[9]}]
set_property IOSTANDARD LVCMOS33 [get_ports {FIXED_IO_mio[8]}]
set_property SLEW SLOW [get_ports {FIXED_IO_mio[8]}]
set_property DRIVE 8 [get_ports {FIXED_IO_mio[8]}]
set_property PIO_DIRECTION OUTPUT [get_ports {FIXED_IO_mio[8]}]
set_property IOSTANDARD LVCMOS33 [get_ports {FIXED_IO_mio[6]}]
set_property SLEW SLOW [get_ports {FIXED_IO_mio[6]}]
set_property DRIVE 8 [get_ports {FIXED_IO_mio[6]}]
set_property PIO_DIRECTION OUTPUT [get_ports {FIXED_IO_mio[6]}]
set_property IOSTANDARD LVCMOS33 [get_ports {FIXED_IO_mio[5]}]
set_property SLEW SLOW [get_ports {FIXED_IO_mio[5]}]
set_property DRIVE 8 [get_ports {FIXED_IO_mio[5]}]
set_property PIO_DIRECTION BIDIR [get_ports {FIXED_IO_mio[5]}]
set_property IOSTANDARD LVCMOS33 [get_ports {FIXED_IO_mio[4]}]
set_property SLEW SLOW [get_ports {FIXED_IO_mio[4]}]
set_property DRIVE 8 [get_ports {FIXED_IO_mio[4]}]
set_property PIO_DIRECTION BIDIR [get_ports {FIXED_IO_mio[4]}]
set_property IOSTANDARD LVCMOS33 [get_ports {FIXED_IO_mio[3]}]
set_property SLEW SLOW [get_ports {FIXED_IO_mio[3]}]
set_property DRIVE 8 [get_ports {FIXED_IO_mio[3]}]
set_property PIO_DIRECTION BIDIR [get_ports {FIXED_IO_mio[3]}]
set_property IOSTANDARD LVCMOS33 [get_ports {FIXED_IO_mio[2]}]
set_property SLEW SLOW [get_ports {FIXED_IO_mio[2]}]
set_property DRIVE 8 [get_ports {FIXED_IO_mio[2]}]
set_property PIO_DIRECTION BIDIR [get_ports {FIXED_IO_mio[2]}]
set_property IOSTANDARD LVCMOS33 [get_ports {FIXED_IO_mio[1]}]
set_property SLEW SLOW [get_ports {FIXED_IO_mio[1]}]
set_property DRIVE 8 [get_ports {FIXED_IO_mio[1]}]
set_property PULLUP true [get_ports {FIXED_IO_mio[1]}]
set_property PIO_DIRECTION OUTPUT [get_ports {FIXED_IO_mio[1]}]
set_property IOSTANDARD LVCMOS33 [get_ports {FIXED_IO_mio[0]}]
set_property SLEW SLOW [get_ports {FIXED_IO_mio[0]}]
set_property DRIVE 8 [get_ports {FIXED_IO_mio[0]}]
set_property PULLUP true [get_ports {FIXED_IO_mio[0]}]
set_property PIO_DIRECTION OUTPUT [get_ports {FIXED_IO_mio[0]}]
set_property IOSTANDARD SSTL15_T_DCI [get_ports FIXED_IO_ddr_vrp]
set_property SLEW FAST [get_ports FIXED_IO_ddr_vrp]
set_property PIO_DIRECTION BIDIR [get_ports FIXED_IO_ddr_vrp]
set_property IOSTANDARD SSTL15_T_DCI [get_ports FIXED_IO_ddr_vrn]
set_property SLEW FAST [get_ports FIXED_IO_ddr_vrn]
set_property PIO_DIRECTION BIDIR [get_ports FIXED_IO_ddr_vrn]
set_property IOSTANDARD SSTL15 [get_ports DDR_we_n]
set_property SLEW SLOW [get_ports DDR_we_n]
set_property PIO_DIRECTION OUTPUT [get_ports DDR_we_n]
set_property IOSTANDARD SSTL15 [get_ports DDR_ras_n]
set_property SLEW SLOW [get_ports DDR_ras_n]
set_property PIO_DIRECTION OUTPUT [get_ports DDR_ras_n]
set_property IOSTANDARD SSTL15 [get_ports DDR_odt]
set_property SLEW SLOW [get_ports DDR_odt]
set_property PIO_DIRECTION OUTPUT [get_ports DDR_odt]
set_property IOSTANDARD SSTL15 [get_ports DDR_reset_n]
set_property SLEW FAST [get_ports DDR_reset_n]
set_property PIO_DIRECTION BIDIR [get_ports DDR_reset_n]
set_property IOSTANDARD DIFF_SSTL15_T_DCI [get_ports {DDR_dqs_p[3]}]
set_property SLEW FAST [get_ports {DDR_dqs_p[3]}]
set_property PIO_DIRECTION BIDIR [get_ports {DDR_dqs_p[3]}]
set_property IOSTANDARD DIFF_SSTL15_T_DCI [get_ports {DDR_dqs_p[2]}]
set_property SLEW FAST [get_ports {DDR_dqs_p[2]}]
set_property PIO_DIRECTION BIDIR [get_ports {DDR_dqs_p[2]}]
set_property IOSTANDARD DIFF_SSTL15_T_DCI [get_ports {DDR_dqs_p[1]}]
set_property SLEW FAST [get_ports {DDR_dqs_p[1]}]
set_property PIO_DIRECTION BIDIR [get_ports {DDR_dqs_p[1]}]
set_property IOSTANDARD DIFF_SSTL15_T_DCI [get_ports {DDR_dqs_p[0]}]
set_property SLEW FAST [get_ports {DDR_dqs_p[0]}]
set_property PIO_DIRECTION BIDIR [get_ports {DDR_dqs_p[0]}]
set_property IOSTANDARD DIFF_SSTL15_T_DCI [get_ports {DDR_dqs_n[3]}]
set_property SLEW FAST [get_ports {DDR_dqs_n[3]}]
set_property PIO_DIRECTION BIDIR [get_ports {DDR_dqs_n[3]}]
set_property IOSTANDARD DIFF_SSTL15_T_DCI [get_ports {DDR_dqs_n[2]}]
set_property SLEW FAST [get_ports {DDR_dqs_n[2]}]
set_property PIO_DIRECTION BIDIR [get_ports {DDR_dqs_n[2]}]
set_property IOSTANDARD DIFF_SSTL15_T_DCI [get_ports {DDR_dqs_n[1]}]
set_property SLEW FAST [get_ports {DDR_dqs_n[1]}]
set_property PIO_DIRECTION BIDIR [get_ports {DDR_dqs_n[1]}]
set_property IOSTANDARD DIFF_SSTL15_T_DCI [get_ports {DDR_dqs_n[0]}]
set_property SLEW FAST [get_ports {DDR_dqs_n[0]}]
set_property PIO_DIRECTION BIDIR [get_ports {DDR_dqs_n[0]}]
set_property IOSTANDARD SSTL15_T_DCI [get_ports {DDR_dq[9]}]
set_property SLEW FAST [get_ports {DDR_dq[9]}]
set_property PIO_DIRECTION BIDIR [get_ports {DDR_dq[9]}]
set_property IOSTANDARD SSTL15_T_DCI [get_ports {DDR_dq[8]}]
set_property SLEW FAST [get_ports {DDR_dq[8]}]
set_property PIO_DIRECTION BIDIR [get_ports {DDR_dq[8]}]
set_property IOSTANDARD SSTL15_T_DCI [get_ports {DDR_dq[7]}]
set_property SLEW FAST [get_ports {DDR_dq[7]}]
set_property PIO_DIRECTION BIDIR [get_ports {DDR_dq[7]}]
set_property IOSTANDARD SSTL15_T_DCI [get_ports {DDR_dq[6]}]
set_property SLEW FAST [get_ports {DDR_dq[6]}]
set_property PIO_DIRECTION BIDIR [get_ports {DDR_dq[6]}]
set_property IOSTANDARD SSTL15_T_DCI [get_ports {DDR_dq[5]}]
set_property SLEW FAST [get_ports {DDR_dq[5]}]
set_property PIO_DIRECTION BIDIR [get_ports {DDR_dq[5]}]
set_property IOSTANDARD SSTL15_T_DCI [get_ports {DDR_dq[4]}]
set_property SLEW FAST [get_ports {DDR_dq[4]}]
set_property PIO_DIRECTION BIDIR [get_ports {DDR_dq[4]}]
set_property IOSTANDARD SSTL15_T_DCI [get_ports {DDR_dq[3]}]
set_property SLEW FAST [get_ports {DDR_dq[3]}]
set_property PIO_DIRECTION BIDIR [get_ports {DDR_dq[3]}]
set_property IOSTANDARD SSTL15_T_DCI [get_ports {DDR_dq[31]}]
set_property SLEW FAST [get_ports {DDR_dq[31]}]
set_property PIO_DIRECTION BIDIR [get_ports {DDR_dq[31]}]
set_property IOSTANDARD SSTL15_T_DCI [get_ports {DDR_dq[30]}]
set_property SLEW FAST [get_ports {DDR_dq[30]}]
set_property PIO_DIRECTION BIDIR [get_ports {DDR_dq[30]}]
set_property IOSTANDARD SSTL15_T_DCI [get_ports {DDR_dq[2]}]
set_property SLEW FAST [get_ports {DDR_dq[2]}]
set_property PIO_DIRECTION BIDIR [get_ports {DDR_dq[2]}]
set_property IOSTANDARD SSTL15_T_DCI [get_ports {DDR_dq[29]}]
set_property SLEW FAST [get_ports {DDR_dq[29]}]
set_property PIO_DIRECTION BIDIR [get_ports {DDR_dq[29]}]
set_property IOSTANDARD SSTL15_T_DCI [get_ports {DDR_dq[28]}]
set_property SLEW FAST [get_ports {DDR_dq[28]}]
set_property PIO_DIRECTION BIDIR [get_ports {DDR_dq[28]}]
set_property IOSTANDARD SSTL15_T_DCI [get_ports {DDR_dq[27]}]
set_property SLEW FAST [get_ports {DDR_dq[27]}]
set_property PIO_DIRECTION BIDIR [get_ports {DDR_dq[27]}]
set_property IOSTANDARD SSTL15_T_DCI [get_ports {DDR_dq[26]}]
set_property SLEW FAST [get_ports {DDR_dq[26]}]
set_property PIO_DIRECTION BIDIR [get_ports {DDR_dq[26]}]
set_property IOSTANDARD SSTL15_T_DCI [get_ports {DDR_dq[25]}]
set_property SLEW FAST [get_ports {DDR_dq[25]}]
set_property PIO_DIRECTION BIDIR [get_ports {DDR_dq[25]}]
set_property IOSTANDARD SSTL15_T_DCI [get_ports {DDR_dq[24]}]
set_property SLEW FAST [get_ports {DDR_dq[24]}]
set_property PIO_DIRECTION BIDIR [get_ports {DDR_dq[24]}]
set_property IOSTANDARD SSTL15_T_DCI [get_ports {DDR_dq[23]}]
set_property SLEW FAST [get_ports {DDR_dq[23]}]
set_property PIO_DIRECTION BIDIR [get_ports {DDR_dq[23]}]
set_property IOSTANDARD SSTL15_T_DCI [get_ports {DDR_dq[22]}]
set_property SLEW FAST [get_ports {DDR_dq[22]}]
set_property PIO_DIRECTION BIDIR [get_ports {DDR_dq[22]}]
set_property IOSTANDARD SSTL15_T_DCI [get_ports {DDR_dq[21]}]
set_property SLEW FAST [get_ports {DDR_dq[21]}]
set_property PIO_DIRECTION BIDIR [get_ports {DDR_dq[21]}]
set_property IOSTANDARD SSTL15_T_DCI [get_ports {DDR_dq[20]}]
set_property SLEW FAST [get_ports {DDR_dq[20]}]
set_property PIO_DIRECTION BIDIR [get_ports {DDR_dq[20]}]
set_property IOSTANDARD SSTL15_T_DCI [get_ports {DDR_dq[1]}]
set_property SLEW FAST [get_ports {DDR_dq[1]}]
set_property PIO_DIRECTION BIDIR [get_ports {DDR_dq[1]}]
set_property IOSTANDARD SSTL15_T_DCI [get_ports {DDR_dq[19]}]
set_property SLEW FAST [get_ports {DDR_dq[19]}]
set_property PIO_DIRECTION BIDIR [get_ports {DDR_dq[19]}]
set_property IOSTANDARD SSTL15_T_DCI [get_ports {DDR_dq[18]}]
set_property SLEW FAST [get_ports {DDR_dq[18]}]
set_property PIO_DIRECTION BIDIR [get_ports {DDR_dq[18]}]
set_property IOSTANDARD SSTL15_T_DCI [get_ports {DDR_dq[17]}]
set_property SLEW FAST [get_ports {DDR_dq[17]}]
set_property PIO_DIRECTION BIDIR [get_ports {DDR_dq[17]}]
set_property IOSTANDARD SSTL15_T_DCI [get_ports {DDR_dq[16]}]
set_property SLEW FAST [get_ports {DDR_dq[16]}]
set_property PIO_DIRECTION BIDIR [get_ports {DDR_dq[16]}]
set_property IOSTANDARD SSTL15_T_DCI [get_ports {DDR_dq[15]}]
set_property SLEW FAST [get_ports {DDR_dq[15]}]
set_property PIO_DIRECTION BIDIR [get_ports {DDR_dq[15]}]
set_property IOSTANDARD SSTL15_T_DCI [get_ports {DDR_dq[14]}]
set_property SLEW FAST [get_ports {DDR_dq[14]}]
set_property PIO_DIRECTION BIDIR [get_ports {DDR_dq[14]}]
set_property IOSTANDARD SSTL15_T_DCI [get_ports {DDR_dq[13]}]
set_property SLEW FAST [get_ports {DDR_dq[13]}]
set_property PIO_DIRECTION BIDIR [get_ports {DDR_dq[13]}]
set_property IOSTANDARD SSTL15_T_DCI [get_ports {DDR_dq[12]}]
set_property SLEW FAST [get_ports {DDR_dq[12]}]
set_property PIO_DIRECTION BIDIR [get_ports {DDR_dq[12]}]
set_property IOSTANDARD SSTL15_T_DCI [get_ports {DDR_dq[11]}]
set_property SLEW FAST [get_ports {DDR_dq[11]}]
set_property PIO_DIRECTION BIDIR [get_ports {DDR_dq[11]}]
set_property IOSTANDARD SSTL15_T_DCI [get_ports {DDR_dq[10]}]
set_property SLEW FAST [get_ports {DDR_dq[10]}]
set_property PIO_DIRECTION BIDIR [get_ports {DDR_dq[10]}]
set_property IOSTANDARD SSTL15_T_DCI [get_ports {DDR_dq[0]}]
set_property SLEW FAST [get_ports {DDR_dq[0]}]
set_property PIO_DIRECTION BIDIR [get_ports {DDR_dq[0]}]
set_property IOSTANDARD SSTL15_T_DCI [get_ports {DDR_dm[3]}]
set_property SLEW FAST [get_ports {DDR_dm[3]}]
set_property PIO_DIRECTION BIDIR [get_ports {DDR_dm[3]}]
set_property IOSTANDARD SSTL15_T_DCI [get_ports {DDR_dm[2]}]
set_property SLEW FAST [get_ports {DDR_dm[2]}]
set_property PIO_DIRECTION BIDIR [get_ports {DDR_dm[2]}]
set_property IOSTANDARD SSTL15_T_DCI [get_ports {DDR_dm[1]}]
set_property SLEW FAST [get_ports {DDR_dm[1]}]
set_property PIO_DIRECTION BIDIR [get_ports {DDR_dm[1]}]
set_property IOSTANDARD SSTL15_T_DCI [get_ports {DDR_dm[0]}]
set_property SLEW FAST [get_ports {DDR_dm[0]}]
set_property PIO_DIRECTION BIDIR [get_ports {DDR_dm[0]}]
set_property IOSTANDARD SSTL15 [get_ports DDR_cs_n]
set_property SLEW SLOW [get_ports DDR_cs_n]
set_property PIO_DIRECTION OUTPUT [get_ports DDR_cs_n]
set_property IOSTANDARD SSTL15 [get_ports DDR_cke]
set_property SLEW SLOW [get_ports DDR_cke]
set_property PIO_DIRECTION OUTPUT [get_ports DDR_cke]
set_property IOSTANDARD DIFF_SSTL15 [get_ports DDR_ck_p]
set_property SLEW FAST [get_ports DDR_ck_p]
set_property PIO_DIRECTION INPUT [get_ports DDR_ck_p]
set_property IOSTANDARD DIFF_SSTL15 [get_ports DDR_ck_n]
set_property SLEW FAST [get_ports DDR_ck_n]
set_property PIO_DIRECTION INPUT [get_ports DDR_ck_n]
set_property IOSTANDARD SSTL15 [get_ports DDR_cas_n]
set_property SLEW SLOW [get_ports DDR_cas_n]
set_property PIO_DIRECTION OUTPUT [get_ports DDR_cas_n]
set_property IOSTANDARD SSTL15 [get_ports {DDR_ba[2]}]
set_property SLEW SLOW [get_ports {DDR_ba[2]}]
set_property PIO_DIRECTION OUTPUT [get_ports {DDR_ba[2]}]
set_property IOSTANDARD SSTL15 [get_ports {DDR_ba[1]}]
set_property SLEW SLOW [get_ports {DDR_ba[1]}]
set_property PIO_DIRECTION OUTPUT [get_ports {DDR_ba[1]}]
set_property IOSTANDARD SSTL15 [get_ports {DDR_ba[0]}]
set_property SLEW SLOW [get_ports {DDR_ba[0]}]
set_property PIO_DIRECTION OUTPUT [get_ports {DDR_ba[0]}]
set_property IOSTANDARD SSTL15 [get_ports {DDR_addr[9]}]
set_property SLEW SLOW [get_ports {DDR_addr[9]}]
set_property PIO_DIRECTION OUTPUT [get_ports {DDR_addr[9]}]
set_property IOSTANDARD SSTL15 [get_ports {DDR_addr[8]}]
set_property SLEW SLOW [get_ports {DDR_addr[8]}]
set_property PIO_DIRECTION OUTPUT [get_ports {DDR_addr[8]}]
set_property IOSTANDARD SSTL15 [get_ports {DDR_addr[7]}]
set_property SLEW SLOW [get_ports {DDR_addr[7]}]
set_property PIO_DIRECTION OUTPUT [get_ports {DDR_addr[7]}]
set_property IOSTANDARD SSTL15 [get_ports {DDR_addr[6]}]
set_property SLEW SLOW [get_ports {DDR_addr[6]}]
set_property PIO_DIRECTION OUTPUT [get_ports {DDR_addr[6]}]
set_property IOSTANDARD SSTL15 [get_ports {DDR_addr[5]}]
set_property SLEW SLOW [get_ports {DDR_addr[5]}]
set_property PIO_DIRECTION OUTPUT [get_ports {DDR_addr[5]}]
set_property IOSTANDARD SSTL15 [get_ports {DDR_addr[4]}]
set_property SLEW SLOW [get_ports {DDR_addr[4]}]
set_property PIO_DIRECTION OUTPUT [get_ports {DDR_addr[4]}]
set_property IOSTANDARD SSTL15 [get_ports {DDR_addr[3]}]
set_property SLEW SLOW [get_ports {DDR_addr[3]}]
set_property PIO_DIRECTION OUTPUT [get_ports {DDR_addr[3]}]
set_property IOSTANDARD SSTL15 [get_ports {DDR_addr[2]}]
set_property SLEW SLOW [get_ports {DDR_addr[2]}]
set_property PIO_DIRECTION OUTPUT [get_ports {DDR_addr[2]}]
set_property IOSTANDARD SSTL15 [get_ports {DDR_addr[1]}]
set_property SLEW SLOW [get_ports {DDR_addr[1]}]
set_property PIO_DIRECTION OUTPUT [get_ports {DDR_addr[1]}]
set_property IOSTANDARD SSTL15 [get_ports {DDR_addr[14]}]
set_property SLEW SLOW [get_ports {DDR_addr[14]}]
set_property PIO_DIRECTION OUTPUT [get_ports {DDR_addr[14]}]
set_property IOSTANDARD SSTL15 [get_ports {DDR_addr[13]}]
set_property SLEW SLOW [get_ports {DDR_addr[13]}]
set_property PIO_DIRECTION OUTPUT [get_ports {DDR_addr[13]}]
set_property IOSTANDARD SSTL15 [get_ports {DDR_addr[12]}]
set_property SLEW SLOW [get_ports {DDR_addr[12]}]
set_property PIO_DIRECTION OUTPUT [get_ports {DDR_addr[12]}]
set_property IOSTANDARD SSTL15 [get_ports {DDR_addr[11]}]
set_property SLEW SLOW [get_ports {DDR_addr[11]}]
set_property PIO_DIRECTION OUTPUT [get_ports {DDR_addr[11]}]
set_property IOSTANDARD SSTL15 [get_ports {DDR_addr[10]}]
set_property SLEW SLOW [get_ports {DDR_addr[10]}]
set_property PIO_DIRECTION OUTPUT [get_ports {DDR_addr[10]}]
set_property IOSTANDARD SSTL15 [get_ports {DDR_addr[0]}]
set_property SLEW SLOW [get_ports {DDR_addr[0]}]
set_property PIO_DIRECTION OUTPUT [get_ports {DDR_addr[0]}]
set_property IOSTANDARD LVCMOS33 [get_ports FIXED_IO_ps_porb]
set_property SLEW FAST [get_ports FIXED_IO_ps_porb]
set_property IOSTANDARD LVCMOS18 [get_ports FIXED_IO_ps_srstb]
set_property SLEW FAST [get_ports FIXED_IO_ps_srstb]
set_property IOSTANDARD LVCMOS33 [get_ports FIXED_IO_ps_clk]
set_property PACKAGE_PIN K22 [get_ports {DDR_addr[0]}]
set_property PACKAGE_PIN K20 [get_ports {DDR_addr[1]}]
set_property PACKAGE_PIN N21 [get_ports {DDR_addr[2]}]
set_property PACKAGE_PIN L22 [get_ports {DDR_addr[3]}]
set_property PACKAGE_PIN M20 [get_ports {DDR_addr[4]}]
set_property PACKAGE_PIN N22 [get_ports {DDR_addr[5]}]
set_property PACKAGE_PIN L20 [get_ports {DDR_addr[6]}]
set_property PACKAGE_PIN J21 [get_ports {DDR_addr[7]}]
set_property PACKAGE_PIN T20 [get_ports {DDR_addr[8]}]
set_property PACKAGE_PIN U20 [get_ports {DDR_addr[9]}]
set_property PACKAGE_PIN M22 [get_ports {DDR_addr[10]}]
set_property PACKAGE_PIN H21 [get_ports {DDR_addr[11]}]
set_property PACKAGE_PIN P20 [get_ports {DDR_addr[12]}]
set_property PACKAGE_PIN J20 [get_ports {DDR_addr[13]}]
set_property PACKAGE_PIN R20 [get_ports {DDR_addr[14]}]
set_property PACKAGE_PIN U22 [get_ports {DDR_ba[0]}]
set_property PACKAGE_PIN T22 [get_ports {DDR_ba[1]}]
set_property PACKAGE_PIN R22 [get_ports {DDR_ba[2]}]
set_property PACKAGE_PIN Y23 [get_ports DDR_cas_n]
set_property PACKAGE_PIN P21 [get_ports DDR_ck_n]
set_property PACKAGE_PIN R21 [get_ports DDR_ck_p]
set_property PACKAGE_PIN U21 [get_ports DDR_cke]
set_property PACKAGE_PIN Y21 [get_ports DDR_cs_n]
set_property PACKAGE_PIN G24 [get_ports {DDR_dm[0]}]
set_property PACKAGE_PIN K25 [get_ports {DDR_dm[1]}]
set_property PACKAGE_PIN P26 [get_ports {DDR_dm[2]}]
set_property PACKAGE_PIN V26 [get_ports {DDR_dm[3]}]
set_property PACKAGE_PIN J26 [get_ports {DDR_dq[0]}]
set_property PACKAGE_PIN F25 [get_ports {DDR_dq[1]}]
set_property PACKAGE_PIN J25 [get_ports {DDR_dq[2]}]
set_property PACKAGE_PIN G26 [get_ports {DDR_dq[3]}]
set_property PACKAGE_PIN H26 [get_ports {DDR_dq[4]}]
set_property PACKAGE_PIN H23 [get_ports {DDR_dq[5]}]
set_property PACKAGE_PIN J24 [get_ports {DDR_dq[6]}]
set_property PACKAGE_PIN J23 [get_ports {DDR_dq[7]}]
set_property PACKAGE_PIN K26 [get_ports {DDR_dq[8]}]
set_property PACKAGE_PIN L23 [get_ports {DDR_dq[9]}]
set_property PACKAGE_PIN M26 [get_ports {DDR_dq[10]}]
set_property PACKAGE_PIN K23 [get_ports {DDR_dq[11]}]
set_property PACKAGE_PIN M25 [get_ports {DDR_dq[12]}]
set_property PACKAGE_PIN N24 [get_ports {DDR_dq[13]}]
set_property PACKAGE_PIN M24 [get_ports {DDR_dq[14]}]
set_property PACKAGE_PIN N23 [get_ports {DDR_dq[15]}]
set_property PACKAGE_PIN R26 [get_ports {DDR_dq[16]}]
set_property PACKAGE_PIN P24 [get_ports {DDR_dq[17]}]
set_property PACKAGE_PIN N26 [get_ports {DDR_dq[18]}]
set_property PACKAGE_PIN P23 [get_ports {DDR_dq[19]}]
set_property PACKAGE_PIN T24 [get_ports {DDR_dq[20]}]
set_property PACKAGE_PIN T25 [get_ports {DDR_dq[21]}]
set_property PACKAGE_PIN T23 [get_ports {DDR_dq[22]}]
set_property PACKAGE_PIN R23 [get_ports {DDR_dq[23]}]
set_property PACKAGE_PIN V24 [get_ports {DDR_dq[24]}]
set_property PACKAGE_PIN U26 [get_ports {DDR_dq[25]}]
set_property PACKAGE_PIN U24 [get_ports {DDR_dq[26]}]
set_property PACKAGE_PIN U25 [get_ports {DDR_dq[27]}]
set_property PACKAGE_PIN W26 [get_ports {DDR_dq[28]}]
set_property PACKAGE_PIN Y25 [get_ports {DDR_dq[29]}]
set_property PACKAGE_PIN Y26 [get_ports {DDR_dq[30]}]
set_property PACKAGE_PIN W23 [get_ports {DDR_dq[31]}]
set_property PACKAGE_PIN G25 [get_ports {DDR_dqs_n[0]}]
set_property PACKAGE_PIN L25 [get_ports {DDR_dqs_n[1]}]
set_property PACKAGE_PIN R25 [get_ports {DDR_dqs_n[2]}]
set_property PACKAGE_PIN W25 [get_ports {DDR_dqs_n[3]}]
set_property PACKAGE_PIN H24 [get_ports {DDR_dqs_p[0]}]
set_property PACKAGE_PIN L24 [get_ports {DDR_dqs_p[1]}]
set_property PACKAGE_PIN P25 [get_ports {DDR_dqs_p[2]}]
set_property PACKAGE_PIN W24 [get_ports {DDR_dqs_p[3]}]
set_property PACKAGE_PIN Y22 [get_ports DDR_odt]
set_property PACKAGE_PIN V23 [get_ports DDR_ras_n]
set_property PACKAGE_PIN H22 [get_ports DDR_reset_n]
set_property PACKAGE_PIN V22 [get_ports DDR_we_n]
set_property PACKAGE_PIN V21 [get_ports FIXED_IO_ddr_vrn]
set_property PACKAGE_PIN W21 [get_ports FIXED_IO_ddr_vrp]
set_property PACKAGE_PIN E26 [get_ports {FIXED_IO_mio[0]}]
set_property PACKAGE_PIN D26 [get_ports {FIXED_IO_mio[1]}]
set_property PACKAGE_PIN E25 [get_ports {FIXED_IO_mio[2]}]
set_property PACKAGE_PIN D25 [get_ports {FIXED_IO_mio[3]}]
set_property PACKAGE_PIN F24 [get_ports {FIXED_IO_mio[4]}]
set_property PACKAGE_PIN C26 [get_ports {FIXED_IO_mio[5]}]
set_property PACKAGE_PIN F23 [get_ports {FIXED_IO_mio[6]}]
set_property PACKAGE_PIN A24 [get_ports {FIXED_IO_mio[8]}]
set_property PACKAGE_PIN D24 [get_ports {FIXED_IO_mio[9]}]
set_property PACKAGE_PIN A25 [get_ports {FIXED_IO_mio[10]}]
set_property PACKAGE_PIN B26 [get_ports {FIXED_IO_mio[11]}]
set_property PACKAGE_PIN A23 [get_ports {FIXED_IO_mio[12]}]
set_property PACKAGE_PIN B25 [get_ports {FIXED_IO_mio[13]}]
set_property PACKAGE_PIN D23 [get_ports {FIXED_IO_mio[14]}]
set_property PACKAGE_PIN C24 [get_ports {FIXED_IO_mio[15]}]
set_property PACKAGE_PIN G21 [get_ports {FIXED_IO_mio[16]}]
set_property PACKAGE_PIN G17 [get_ports {FIXED_IO_mio[17]}]
set_property PACKAGE_PIN G20 [get_ports {FIXED_IO_mio[18]}]
set_property PACKAGE_PIN G19 [get_ports {FIXED_IO_mio[19]}]
set_property PACKAGE_PIN H19 [get_ports {FIXED_IO_mio[20]}]
set_property PACKAGE_PIN F22 [get_ports {FIXED_IO_mio[21]}]
set_property PACKAGE_PIN G22 [get_ports {FIXED_IO_mio[22]}]
set_property PACKAGE_PIN F20 [get_ports {FIXED_IO_mio[23]}]
set_property PACKAGE_PIN J19 [get_ports {FIXED_IO_mio[24]}]
set_property PACKAGE_PIN F19 [get_ports {FIXED_IO_mio[25]}]
set_property PACKAGE_PIN H17 [get_ports {FIXED_IO_mio[26]}]
set_property PACKAGE_PIN F18 [get_ports {FIXED_IO_mio[27]}]
set_property PACKAGE_PIN J18 [get_ports {FIXED_IO_mio[28]}]
set_property PACKAGE_PIN E20 [get_ports {FIXED_IO_mio[29]}]
set_property PACKAGE_PIN K19 [get_ports {FIXED_IO_mio[30]}]
set_property PACKAGE_PIN E21 [get_ports {FIXED_IO_mio[31]}]
set_property PACKAGE_PIN K17 [get_ports {FIXED_IO_mio[32]}]
set_property PACKAGE_PIN E22 [get_ports {FIXED_IO_mio[33]}]
set_property PACKAGE_PIN J16 [get_ports {FIXED_IO_mio[34]}]
set_property PACKAGE_PIN D19 [get_ports {FIXED_IO_mio[35]}]
set_property PACKAGE_PIN K16 [get_ports {FIXED_IO_mio[36]}]
set_property PACKAGE_PIN D20 [get_ports {FIXED_IO_mio[37]}]
set_property PACKAGE_PIN D21 [get_ports {FIXED_IO_mio[38]}]
set_property PACKAGE_PIN C21 [get_ports {FIXED_IO_mio[39]}]
set_property PACKAGE_PIN C22 [get_ports {FIXED_IO_mio[40]}]
set_property PACKAGE_PIN C19 [get_ports {FIXED_IO_mio[41]}]
set_property PACKAGE_PIN F17 [get_ports {FIXED_IO_mio[42]}]
set_property PACKAGE_PIN D18 [get_ports {FIXED_IO_mio[43]}]
set_property PACKAGE_PIN E18 [get_ports {FIXED_IO_mio[44]}]
set_property PACKAGE_PIN C18 [get_ports {FIXED_IO_mio[45]}]
set_property PACKAGE_PIN B21 [get_ports {FIXED_IO_mio[48]}]
set_property PACKAGE_PIN A18 [get_ports {FIXED_IO_mio[49]}]
set_property PACKAGE_PIN B22 [get_ports {FIXED_IO_mio[50]}]
set_property PACKAGE_PIN B20 [get_ports {FIXED_IO_mio[51]}]
set_property PACKAGE_PIN A20 [get_ports {FIXED_IO_mio[52]}]
set_property PACKAGE_PIN A19 [get_ports {FIXED_IO_mio[53]}]
set_property PACKAGE_PIN B24 [get_ports FIXED_IO_ps_clk]
set_property PACKAGE_PIN C23 [get_ports FIXED_IO_ps_porb]
set_property PACKAGE_PIN A22 [get_ports FIXED_IO_ps_srstb]
set_property SLEW FAST [get_ports FIXED_IO_ps_clk]
